

COMPUTER JARGON ACRYONYMS
(A)

ADT
- 
Abstract data type

AI
- 
Artificial intelligence

ALU
- 
Arithmetic logic unit

API
- 
Application program interface

ASCII
- 
American standards institute

ANSI
- 
American national standard institute

ASI
- 
Accredited standard institute 

ATM
 -
Automatic teller machine

ALGOL- 
ALGOrithmic language

AOSs
- 
Advanced office systems

(B)

BIOS
-    
Basic-input system

BISNYC- 
BINary SYNchronous

BCD
-  
Binary coded decimal

BASIC
- 
Beginners all purpose symbolic instruction code

BTS
- 
Bits per second

(C)

CU
- 
Control unit

CPU
- 
Central processing unit

CD-ROM- 
Compact disk – read only memory

CRT
- 
Cathode ray tube

CAD
- 
Computer aided designing

CAM
- 
Computer aided manufacture

CAE
- 
Computer aided engineering

CPS
- 
Character per second

CISC
- 
Complex instruction set computer

COBOL- 
Commercial business oriented programming language

CASE
- 
Computer aided software engineering

CSMA/CD- 
Carrier- sease multiple access with collision the detection 

CUSDEC- 
CUSItoms DECIaration message 

CGA
- 
Color graphics adaptor

COM
- 
Computer output microfilm

CAL
- 
Computer assisted learning

CP/M
- 
Control programme for microprocessor

CBIS
- 
Computer based information system

(D)

DIP
-
Dual in –line package

DMA
- 
Direct memory access

DTP
- 
Desk top publishing 

DOS
- 
Disk operating system 

DDE
- 
Dynamic data exchange 

DFDs
- 
Data flow diagrams 

DLL
- 
Dynamic link library

DTE
- 
Data terminal equipment

DCTE
- 
Data circuit terminating equipment

DoT
-
Department of telecommunication

DES
-
Data Encription standard

DBMS
- 
Data base management system

DATACOMM
Data communication

DDS
- 
Decision support system 

DD
- 
Data dictionary

(E)

ENIAC- 
Electronic numerical integrator and calculator

EPROM-
Erasable programmable read only memory

EEPROM- 
Electrically erasable programmable read only memory

ERDs
- 
Entity relationship diagrams 

EBCDIC- 
Extended binary decimal interchange code

EDI
- 
Electronic data interchange

E-MAIL- 
Electronic mail

EFT
- 
Electronic fund transfer

EDP
- 
Electronic data processing

ES
- 
Expert system

(F)

FAQ
- 
Frequently asked question

FORTRAN- 
FORmula TRANslation  language

FTP
- 
File transfer protocol

FAT
- 
File allocation table

(G)

GB
- 
Giga bytes

GUI
- 
Graphical user interface

GDI
- 
Graphics device interface

GHz
- 
Giga hertz

GIGO
- 
Garbage- in garbage –out

(H) 

HTML
- 
Hyper text markup language

HDLC
-
Highlevel data link control 

HGA
- 
Hercules graphics array

HAL
- 
Human access language

(I)

IP
- 
Internet protocol

ISOC
- 
Internet SOCiety

IT
-
Information technology

I/O
- 
Input output

IBM
- 
International business machine

Ics
- 
Integrated circuits

IR
- 
Instruction register 

ITTCC
- 
International telegraph & telephone consultative committee

ISDN
- 
Integrated switched data network

ISR’s
- 
Interrupt services routines 

IRGs
- 
Inter record gaps

IAB
- 
Internet architecture board

IETE
- 
Internet engineering task force

(J)

JCL
- 
Job contral language

(K)

KB
- 
Kilo bytes

KBPS
- 
Kilo bits per second

KBS
- 
Knowledge based system


(L)

LSE
- 
Landon school of economics

LSI
- 
Large scale integration

LCD
- 
Liquid crystal display 

LPM
- 
Line per minute

LAN
- 
Local area network

LISP
- 
LISt processing

(M)

MIS
- 
Management information system

MIPS
- 
Million instructior per second

MB
- 
Mega bytes

MAR
- 
Memory address register 

MICR
- 
Magnetic ink character recognition

MISD
- 
Multiple instruction single data

MIMD
- 
Multiple instruction multiple data

MS-DOS- 
Micro soft disk operating system

MODEM- 
Modulator DEModulator

MHz
- 
Mega hertz 

MBPS
- 
Million of bits per second

MA
- 
Multiple access

MDA
- 
Monochrome display adaptor 

(N)

NCSA
- 
National center for supercomputer application

NIC
- 
Network interface card

NIU
- 
Network interface unit

(O)

OOP
-
Object oriented programming

OAS
- 
Office automation system

OLTP
- 
On line transaction processing

OMR
- 
Optical mark reader

OBR
- 
Optical barcode reader

OCR
- 
Optical character recognition

OS
- 
Operating system 

OSI
- 
Open system interconnecting

(P)

PPP
- 
Point to point protocol

PGA
- 
Pin grid array 

PC
- 
Personal computer

PC-XT
- 
Personal computer with extended technology

PC-AT
- 
Personal computer with advanced technology 

PROM
- 
Programmable read only memory

PPM
- 
Page per minute 

PM
- 
Presentation manager

PSDs
- 
Program structure diagram 

PSTN
- 
Public switched telephone network

PSDN
- 
Public switched data network

PSPDNC- 
Package switching public data network card

PINs
- 
Personal identification numbers

POST
- 
Power of self test

POF
- 
Portable document file

(R)

RAM
- 
Random access memory 

ROM
- 
Read only memory

RISC
- 
Reduced instruction set computer

RDBMS- 
Relational data base management system

RPM
- 
Revolution per minute

(S)

SSI
- 
Small scale integration 

SISD
- 
Single instruction single data

SIMD
- 
Single instruction multiple data

SQL
- 
Sequential query language 

SAA
- 
System application architecture

SDLC
- 
System development life cycle

SNOBOL- 
String oriented symbolic language 

SLIP
-
Serial line internet protocol

(T)

TCP
- 
Transmission  control protocol

TPS
- 
Transaction processing systems

TB
- 
Terra bytes

TDI
- 
Trade data interchange

(U)
UCS
- 
Uniform communication standard

(V)

VB
- 
Visual basic 

VLSI
- 
Very large scale integration 

VDU
- 
Visual display unit

VAN
- 
Value aided network 

VGA
- 
Video graphics array

VSNL
- 
Videsh sanchar nigam limited

(W)

WWW
- 
World wide web

WAIS
- 
Wide area information server

WYSIWYG – 
What you see is what you get 

WAN
- 
Wide area network

